# NOTICE

**on the purchase of**

**USED BUSES**

**1. Name of the beneficiary: Municipal Enterprise “Urban Bus Park”**

**2. IDNO: 1004600054327**

**3. Address: Chișinău Municipality, 51 Sarmizegetusa Street**

**4. Telephone / fax number: 022-83-73-35/022-55-60-30**

**5. Beneficiary's e-mail and internet address: info@autourban.md/www.autourban.md**

**6. E-mail or internet address from which it will be possible to obtain access to the specifications: the specifications are attached during the procedure on the page: *www.achiziții.md; www.autourban.md; www.chisinau.md.***

**7. Type of beneficiary and main object of activity: urban passenger transport.**

**8. Type of procurement procedure: direct procurement**

**9. Code CPV – 34121100-2**

**10. The buyer invites interested economic operators, who can meet the needs, to participate in the procedure for the purchase of buses in accordance with the following technical specifications:**

**Buses 12M**

|  |  |  |
| --- | --- | --- |
| No. | **Article name** | **Requirements** |
| 1 | **General characteristics** | |
| 2 | Year of production | From 1 July 2013 (alternatively 1 July 2011) ⃰ |
| 3 | Distance km | ≤400000 (alternatively 500000)⃰ |
| 4 | Vehicle category | Bus for passenger transport on urban and suburban routes, at an ambient temperature of minus 35 ° C to plus 45 ° C |
| 5 | Ecological class | EURO 5-6 |
| 6 | Total capacity, passengers | ≥100 |
| 7 | Number of seats | ≥22 |
| 8 | Overall dimensions:  - length, mm  - width, mm  - height, mm | 12000-14500  maximum 2550  maximum 3300 |
| 9 | Floor level | low-floor |
| 10 | The formula of the doors | 2+2+2 |
| 11 | Flooring | Resistant to wear and rot |
| 12 | Ventilation and heating system: | Air conditioning system  At least 2 ventipans on the roof of the bus.  At least 4 windows.  Driver's cab heating with autonomous heating |
| 13 | The driver's space | Cabin - separated from the passengers by a partition wall |
| 14 | Information system | Electronic informant (front, side, back, salon) |
| 15 | Engine | Four-stroke turbocharged diesel engine. |
| 16 | Gearbox | Automatic |
| 17 | Additional facilities | Folding ramp for disabled access, comfortable chairs. |

**Buses 9M**

|  |  |  |
| --- | --- | --- |
| No. | **Article name** | **Requirements** |
| 1 | **General characteristics** | |
| 2 | Year of production | From 1 July 2013 (alternatively 1 July 2011) ⃰ |
| 3 | Distance km | ≤400000 (alternatively 500000)⃰ |
| 4 | Vehicle category | Bus for passenger transport on urban and suburban routes, at an ambient temperature of minus 35 ° C to plus 45 ° C |
| 5 | Ecological class | EURO 5-6 |
| 6 | Total capacity, passengers | ≥69 |
| 7 | Number of seats | ≥22 |
| 8 | Overall dimensions:  - length, mm  - width, mm  - height, mm | ≤9500  maximum 2550  maximum 3300 |
| 9 | Floor level | low-floor |
| 10 | The formula of the doors | 2+2 |
| 11 | Flooring | Resistant to wear and rot |
| 12 | Ventilation and heating system: | Air conditioning system  At least 2 ventipans on the roof of the bus.  At least 4 windows.  Driver's cab heating with autonomous heating |
| 13 | The driver's space | Cabin - separated from the passengers by a partition wall |
| 14 | Information system | Electronic informant (front, side, back, salon) |
| 15 | Engine | Four-stroke turbocharged diesel engine. |
| 16 | Gearbox | Automatic |
| 17 | Additional facilities | Folding ramp for disabled access, comfortable chairs. |

**Buses 18M**

|  |  |  |
| --- | --- | --- |
| No. | **Article name** | **Requirements** |
| 1 | **General characteristics** | |
| 2 | Year of production | From 1 July 2013 (alternatively 1 July 2011) ⃰ |
| 3 | Distance km | ≤400000 (alternatively 500000)⃰ |
| 4 | Vehicle category | Bus for passenger transport on urban and suburban routes, at an ambient temperature of minus 35 ° C to plus 45 ° C |
| 5 | Ecological class | EURO 5-6 |
| 6 | Total capacity, passengers | ≥150 |
| 7 | Number of seats | ≥35 |
| 8 | Overall dimensions:  - length, mm  - width, mm  - height, mm | 17600-18400  maximum 2550  maximum 3300 |
| 9 | Floor level | Low-flood |
| 10 | The formula of the doors | 2+2+2+2 |
| 11 | Flooring | Resistant to wear and rot |
| 12 | Ventilation and heating system: | Air conditioning system  At least 3 ventipans on the roof of the bus.  At least 6 windows.  Driver's cab heating with autonomous heating |
| 13 | The driver's space | Cabin - separated from the passengers by a partition wall |
| 14 | Information system | Electronic informant (front, side, back, salon) |
| 15 | Engine | Four-stroke turbocharged diesel engine. |
| 16 | Gearbox | Automatic |
| 17 | Additional facilities | Folding ramp for disabled access, comfortable chairs. |

**11. Quantity of buses required - within the available stock of the bidder and within the available budget of the beneficiary.**

**12. Available budget of the beneficiary - 50,000,000.0 lei with VAT**

**13. Admission or prohibition of alternative offers: Admitted.**

**14. Required delivery terms and conditions: 30 days from the signing of the contract.**

**15. The term of validity of the contract: \_12 months.**

**16. Procurement contract reserved for sheltered workshops or may be performed only under sheltered employment programs (where applicable): yes.**

**17. Necessary documents to present:**

|  |  |  |  |
| --- | --- | --- | --- |
| **No.** | **Description of the criterion / requirement** | **How to demonstrate the fulfillment of the criterion / requirement:** | **Minimum level /**  **mandatory** |
| 1 | Proof of registration of the legal entity | Extract from the State Register of legal entities (not older than 6 months) - copy, confirmed by applying the bidder's signature and stamp. | YES |
| 2 | Offer form | Original - Confirmed by the Participant's signature and stamp | YES |
| 3 | Price specification and technical specifications | Confirmed by the Participant's signature and stamp | YES |
| 4 | Bus warranty period (optional, if applicable) | Original - Confirmed by the Participant's signature and stamp | NO |
| 5 | Bus technical expertise report | Original - Developed by a licensed independent institution | YES |

**18. Special conditions on which performance of the contract depends: Not applicable.**

**19. Evaluation criterion applied for the award of the contract: The best technical-economic offer. Following the examination of the submitted bids, the beneficiary may award the procurement contracts to several economic operators and only to those buses that have met all the required technical-economic criteria.**

**20. Deadline for submission / opening of tenders:**

**- until: [exact time] According to www.achizitii.md**

**- on: [date] according to** [**www.achizitii.md**](http://www.achizitii.md)

**21. Address to which tenders or requests to participate must be sent:**

**Chișinău Municipality, 51 Sarmizegetusa Street, offoce 302,** [**info@autourban.md**](mailto:info@autourban.md)**,** [**autobuze@pmc.md**](mailto:autobuze@pmc.md)

**22. The term of validity of the offers: 30 days.**