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CAIET DE SARCINI
PENTRU  CEREREA OFERTEI  DE  PREŢ

Introducere: 
Caietul de sarcini face parte integrantă din documentaţia pentru atribuirea contractului şi 
constituie ansamblul cerinţelor pe baza cărora se elaborează de către fiecare ofertant 
propunerea tehnică. Caietul de sarcini conţine specificaţii tehnice, care vor fi considerate ca 
fiind minimale. În acest sens, orice ofertă prezentată, care se abate de la prevederile Caietului de sarcini, va fi luată în considerare, dar numai în măsura în care propunerea tehnică presupune asigurarea unui nivel calitativ superior cerinţelor minimale din Caietul de sarcini. Ofertele care nu satisfac cerinţele caietului de sarcini vor fi declarate oferte neconforme şi vor fi respinse.
Denumirea achiziției: Achiziționarea și montarea sistemului de supraveghere video și sistem de limitare a accesului pe teritoriul și în incinta la Liceul Teoretic cu profil de arte "Elena Alistar" amplasat pe Bd. Decebal 74. 
Amplasarea obiectului:                                                                                                                                                                                         Mun. Chisinau, Sector Botanica Bd. Decebal nr. 74
1. Termenul de efectuare: 40 zile calendaristice din momentul semnării contractului.
2. Modul de finalizare a lucrărilor: Executantul este dator să notifice investitorului data terminării tuturor lucrărilor prevăzute în contract, printr-un document scris, confirmat de reprezentantul investitorului pe șantier, pentru desemnarea comisiei de recepție la terminarea lucrărilor.
3. Documentația de referință:
5.1.  Planul Cadastral:
5.2. Normativele în vigoare privind sistemele de securitate. 
 6. Cerințe de bază: 
6.1. Participanții asigură efectuarea luсrărilоr în conformitate cu Codul urbanistic .
6.2. Împreună cu sistemul să fie livrate accesoriile necesare instalării.
6.3. Toate cerinţele tehnice sunt minimale şi obligatorii. Toate echipamentele ofertate trebuie să fie compatibile cu standardele de alimentare cu energie electrică disponibile în Moldova: 220V c.a.  la 50 Hz. Toate echipamentele ofertate trebuie să fie noi şi neutilizate anterior. Ofertanţii vor include în ofertă, în original, un document emis de către producătorul echipamentelor ofertate care să certifice că modelele echipamentelor ofertate sunt în producţie (nu sunt declarate EOL) la data ofertei.
6.4. Operatorul economic adjudecat câștigător este obligat să aprobe, avizeze și coordoneze execuția lucrărilor, darea lor în exploatare cu Beneficiarul, autoritățile și instanțele de resort.
Operatorii economici participanti la licitatie trebuie sa detie Certificat MAF( Manufacturer Authorization Form) de la producatorul de echipament, si centru de deservire sau contract cu centrul de deservire autorizat de producator. 
6.5. Ofertantul are obligația de a executa lucrările cu folosirea materialelor certificate în RM.
6.6. Tot utilajul trebuie să fie certificat, precum şi să dispună de toată documentația tehnică (specificaţia, descrierea, instrucțiuni pentru utilizatori).
6.7. Toate deficiențele, viciile apărute în pe parcursul termenului de garanție vor fi remediate de către Ofertant imediat, dar nu mai târziu de 15 (cincisprezece) zile lucrătoare de la momentul notificării. 
6.8. [bookmark: _Hlk177635330]Ofertantul se obligă să execute toate lucrările și volumele incluse în caietul de sarcini și proiectele de execuție. 
6.9. Vizitarea obiectivului supus îndeplinirii lucrărilor din caietul de sarcini, corespunderea caietului de sarcini și volumele de lucrări, sресifiсând data cînd acesta a făcut cunoștință cu locul (obiectul) efectuării luсrărilоr. În cazul depistării lucrărilor neprevăzute sau neconformități a caitului de sarcini cu lucrările ce urmează a fi îndeplinite ofertantul este obligat să înștiințeze Beneficiarul în scris în termeni cît mai restrînși pentru clarificări.
6.10. Ofertantul garantează calitatea lucrărilor îndeplinite în termen de 2 ani din data semnării Procesului-Verbal de recepție la terminarea lucrărilor și înlătură defectele pe tot termenul de garanție din cont propriu dacă acestea sunt legate de nerespectarea normelor în vigoare și regulilor tehnice pe parcursul îndeplinirii lucrărilor sau de calitatea materialelor folosite.
6.11. Termenul de garanție pentru toate echipamentele de baza furnizate trebuie să fie minim de 36 de luni din data semnării Procesului-Verbal de recepție. 
6.12. Autoritatea contractantă nu efectuează plăți anticipate în calitate de avans. 
6.13. Achitarea lucrărilor executate se va efectua de către Autoritatea contractantă în baza procesului-verbal de executare a lucrărilor și facturii fiscale în termen de 10 zile calendaristice din data înregistrării facturii fiscale  în registrul Beneficiarului. Executantul lucrărilor va emite factura fiscală Beneficiarului în termen de 5 zile calendaristice după semnarea de către părți a Procesului-Verbal de executare a lucrărilor și/sau Actului de recepție finală a lucrărilor.
6.14. Ofertele vor fi prezentate cu semnătură și ștampilă autorizată a firmei.
6.15. Lista materialelor și echipamentelor, conform proiectului, sunt indicate în Anexa nr.1, parte a acestui document.  
7. Ofertantul prezintă actele confirmative care atestă dreptul de activitate inclusiv executarea lucrărilor în domeniul respectiv.
8. Operatorii economici vor avea acces la toate cabinetele si documentatiile tehnice detinute de beneficiar pe durata executarii lucrarilor. 

Anexa nr. 1
[bookmark: _Hlk177632309][bookmark: _Hlk175045867]Sistemul supraveghere video 
[bookmark: _Hlk176265007]
	Nr.crt.
	Denumirea Utilajului si a Materialelor
	Unitatea de masura
	Volum

	
	Cabluri
	
	

	1. 
	Cablu extern FTP Cat.6 4P CU Solid Outdoor, cu tross de susținere, HF (Halogen Free)
Cablu FTP Categoria 6 destinat instalațiilor exterioare, prevăzut cu 4 perechi torsadate și ecranaj general din folie de aluminiu pentru protecție împotriva interferențelor electromagnetice (EMI). Conductori realizați din cupru masiv (Solid Copper) cu diametrul de 0,57 mm (23 AWG). Echipat cu tross metalic integrat pentru montaj aerian și susținere mecanică suplimentară.
	m
	2100

	2. 
	Cablu FTP Cat.6 4P CU, HF ( Halogen Free) Interior
	M
	560

	3. 
	Cablu optic cu 4 Fire  
Atenuare: 1310nm ≤0,36 db/km
Atenuare: 1550nm ≤0,22 db/km
Rezultatul testului: Trecut
	m
	260

	4. 
	Cablu Alimentare  VVGnG 3x1.5 LS
Secțiune 1.5 mm²
Numărul de fire 3 *
Culoare Negru
Tip material Cupru
Temperatura mediului ambiant la exploatare
de la -50°С pînă la +50°С
Temperatura maximă de încalzire a firelor +70°С
	m
	150


	
	Materiale

	5. 
	Materiale de Fixare cablu si echipament
	Set
	50

	6. 
	Conector terminal de fibra optica 2.5
	buc.
	4

	7. 
	Box optic terminal de abonat 1 si 2 fibre (FTTH)
	buc
	2

	8. 
	FO Patch-cord
	buc
	4

	9. 
	SFP module
	buc
	2

	10. 
	Conector RJ-45
	buc
	60

	
	Utilaj Video

	11. 
	8 MP Smart Hybrid Light with ColorVu Fixed Mini Bullet Network Camera
HikAI-ISP for excellant noise reduction effect
24/7 colorful imaging via ColorVu technology
Scene-adaptive WDR
Focus on Person and Vehicle classification based on deep learning
Built-in arrayed dual-microphone for real-time high quality audio security
Provide real-time security via built-in two-way audio
Anti-corrosion design, providing reliability and longevity compared to standard (NEMA4X)
Smart Hybrid Light: Integrates IR and White lights, 3 supplemental lighting modes
Water and dust resistant (IP67)
Active strobe light and audio alarm to warn intruders off
Image Sensor
1/1.8" Progressive Scan CMOS
Max. Resolution 3840 × 2160
Min. Illumination
Color: 0.0005 Lux @ (F1.0, AGC ON),0 Lux with light
Shutter Time 1 s to 1/100,000 s
Day & Night IR cut filter
Angle Adjustment
Pan: 0° to 360°,tilt: 0° to 90°,rotate: 0° to 360°
Deep Learning Function
Face Capture Yes
Perimeter Protection
Line crossing, intrusion, region entrance, region exiting
Support alarm triggering by specified target types (human and vehicle)
Material
Front cover: Metal, body: Metal, bracket: Metal
Power
12 VDC ± 25%, 1.25 A, max. 15 W,Ø5.5 mm coaxial power plug,reverse polarity protection,
PoE: IEEE 802.3at, Class 4, max. 18 W

	buc
	19 

	12. 
	Camera Video pentru Interior cu parametrii minimi 
8 MP Network Turret Camera with Smart Hybrid Light and ColorVu Technology
8 Megapixel network turret camera featuring Smart Hybrid Light technology and 24/7 full-color imaging. Designed for high-quality video surveillance in residential, commercial and industrial applications, providing excellent image clarity in low-light and nighttime conditions.
Intelligent Functions
Human and vehicle classification based on deep learning algorithms
Line crossing detection
Intrusion detection
Region entrance detection
Region exit detection
Motion detection with intelligent filtering
Push alarm notifications to mobile devices
Video
Maximum resolution: 3840 × 2160 (8 MP)
High-performance progressive scan CMOS image sensor
Full-color imaging 24 hours a day
Excellent low-light sensitivity
True WDR 120 dB
BLC, HLC and 3D DNR image enhancement technologies
Multi-stream support
Video compression: H.265+, H.265, H.264+, H.264 and MJPEG
Lens
Fixed focal lens
Wide viewing angle for comprehensive area coverage
Audio
Built-in microphone
High-quality audio recording synchronized with video streams
Illumination
Smart Hybrid Light technology
IR illumination for discreet night monitoring
White light illumination for full-color night imaging
Automatic switching between illumination modes according to scene conditions
Illumination range up to 30 m
Storage and Network
MicroSD/SDHC/SDXC card support (depending on configuration)
Ethernet network interface
Remote access via web browser, software platform and mobile application
Power
12 VDC power supply
PoE (Power over Ethernet) support according to IEEE 802.3af standard
Environmental
IP67-rated weatherproof housing
Suitable for indoor and outdoor installation
Operating temperature range from -30°C to +60°C
Applications
Commercial buildings
Hotels and hospitality facilities
Industrial sites
Educational institutions
Residential complexes
Perimeter and parking area monitoring
Warranty
3-year manufacturer warranty
	Buc
	17

	13. 
	Comutator de retea de 24 porturi cu parametrii minim 
24-Port Smart Monitoring PoE+ Switch for Video Surveillance Networks
Managed Smart Monitoring PoE+ switch designed for IP video surveillance and security network applications. Provides simultaneous data transmission and power delivery over Ethernet with extended transmission distance of up to 300 m in long-range mode.
Ports and Connectivity
24 × 10/100 Mbps PoE+ RJ45 ports
2 × Gigabit Combo ports
Extended PoE transmission distance up to 300 m
Simultaneous power and data transmission over a single Ethernet cable
PoE Features
IEEE 802.3af and IEEE 802.3at compliant
Maximum PoE output per port: 30 W
Total PoE power budget: 370 W
Priority power allocation on ports 1–8
Supports power delivery over Ethernet cable pairs 1/2, 3/6 and 4/5, 7/8
Smart Monitoring Functions
Network topology visualization
Network health monitoring and status overview
Real-time bandwidth and traffic statistics
Port utilization and line load monitoring
Alarm and event notifications
Remote switch reboot capability
Remote individual port restart
Event and system log management
Integrated live camera view support
Performance
Switching capacity: 8.8 Gbps
Optimized for stable video and data transmission
Reliable operation in high-density surveillance deployments
Protection
6 kV surge protection
Enhanced protection against lightning-induced electrical surges
Power Supply
Input voltage: AC 220 V
Environmental
Fanless design for silent operation and increased reliability
Operating temperature: -10°C to +55°C
Physical Characteristics
Dimensions: 440 × 221 × 44 mm
Rack-mountable metal enclosure
Applications
IP video surveillance systems
Security and monitoring networks
Commercial and industrial facilities
Critical infrastructure installations
Building Management Systems (BMS)
Access control and integrated security platforms
Warranty
3-year manufacturer warranty
	Buc
	1

	14. 
	Comutator de retea cu 8 porturi  cu parametrii minim; 
SWITCH POE 
• Switch PoE 8 canale
• Putere totala 110W
• Distanta de transmisie max. 300 metri
• Suporta management de putere PoE 
• 8 Porturi PoE 10/100 Mbps
• 1 Port Ethernet 1000 Mbps 
• 1 Port SFP 1000 Mbps 
	buc
	3 

	15. 
	NVR de 64 canale si 4 spatii pentru HDD pana la 16TB 
 cu parametrii minimi 

H.265+/H.265/H.264+/H.264 video formats
Intelligent analytics based on Guanlan Large-Scale AI Models
Up to 64-ch AcuSeek and AcuSearch function
Up to 8-ch facial recognition for face picture
Up to 64-ch IP camera inputs
Up to 32-ch 1080p decoding capability
Up to 8-ch IP speakers can be connected 
AI by NVR
Facial recognition
AI by NVR and Camera
Facial recognition, perimeter protection, video structuralization, AcuSearch, motion detection 2.0, ANPR, people counting, AcuSeek
Video Output Mode
HDMI1/VGA1 simultaneous output, HDMI2/VGA2 simultaneous output
CVBS Output
NA
Audio Output
2-ch, RCA (Linear, 1 KΩ)
Two-Way Audio
1-ch, RCA (2.0 Vp-p, 1 KΩ)
HDMI 1 Output
4K（3840×2160）/30Hz，2K（2560×1440）/60Hz，1080P（1920×1080）/60Hz，720P（1280×720）/60Hz
Stream Type Video, Video & Audio

	buc
	1

	16. 
	Switch (comutator de rețea)
Layer 3 managed switch
Cantitatea porturilor minimala – 12 
Minim 2 porturi Gigabit Ethernet sau 2 porturi SPF cu module RJ45 Gigabit Ethernet instalate 
Minim 10 porturi Gigabit SFP și/sau 10Gigabit SFP
Suportă implementarea în rețele IPv6 și IPv4
Inspecție ARP, IP Source Guard, protecție DoS, securitate porturi și DHCP Snooping
Controler încorporat pentru gestionarea comutatorului; 
QoS încorporat permite prioritizarea traficului de rețea.
	buc
	1

	17. 
	Unitate de stocare Unitate HDD Western Digital WD 16 TB
Tip unitate de stocare
Unitate HDD
Sistem de stocare a datelor 3.5"
Capacitate memorie 16 TB
Dimensiune memorie tampon (cache) 512 MB
Interfață SSD SATA-3 (6 Gb/s)
	Buc
	4

	18. 
	Calculator Monitorizare Video (set)
Monitor: diagonala 32 inch, rezolutia minima 2K, HDMI, DisplayPort
PC, cerinte minimale: CPU 8 nuclee 3.7 GHz fiecare, placa de baza cu interfate HDMI si DisplayPort, RAM 16 GB, SSD 128 GB, HDD 1000 GB, PSU – 550W
Tastatura USB, Mouse USB
UPS 800VA/480W, Line Interactive, AVR, LED, 2xShuko Sockets
	set
	1

	19. 
	Televizor pentru post de monitorizare 55" LED SMART TV TCL 
	Buc
	1

	
	Surse de Alimentare

	20. 
	Sursa de Alimentare de Rezerva 
Tip UPS: linie interactivă, undă sinusoidală pură
Intrare: 220V AC ± 25%, 50Hz / 60Hz ± 10%
Ieșire: 220V AC ± 10%, 50Hz / 60Hz ± 0,5% (pe baterie)
Prize: intrare IEC C14, ieșiri: Schuko tip EU x 1 buc, IEC C13 x 6 buc
Condiții de funcționare: 0°C~40°C, la umiditate 10~90%RH fără condensare
Zgomot: < 45 dB (la 1 metru distanta)
Putere: 3000 VA (2400 W)
Dimensiuni: 440 x 410 x 132 mm
	buc
	1

	
	Dulapuri si Boxe

	21. 
	Dulap Metalic 800x600x250
	buc
	2

	22. 
	Dulap de Telecomunicatii 
Dulap de perete 9U pentru echipamente de rețea cu ușă frontală blocabilă din sticlă călită, panouri laterale detașabile și deschideri de ventilație pentru răcirea echipamentelor.
Capacitate maximă de încărcare de 60 kg. 
Ușă frontală din sticlă blocabilă. 
Nivel de protecție IP20. 
Lățime - 600 mm, adâncime - 450 mm, înălțime - 501 mm. 
Material - oțel laminat la rece.
	buc
	1

	23. 
	Elemente de Fixare compatibile cu sistemul
	set
	10

	24. 
	Soft de Monitorizare Video+Paza+ Module

	set
	1

	25. 
	Servicii de trasare cabluri, instalare si configurare echipamente. 
	Serv
	1





Sistemul Limitare a accesului integrat cu Sistem Video

	Nr.crt.
	Denumirea Utilajului si a Materialelor
	Unitatea de masura
	Volumul

	
	Utilaj Central
	
	

	1. 
	Centrala de acces Biometrica la intrarile pe teritoriu
Multifactor Biometric Access Control and Time Attendance Terminal with Face Recognition
Advanced biometric access control and time attendance terminal based on deep learning facial recognition technology. Designed for secure identification, workforce management and integration with access control, video surveillance and IP intercom systems.
Authentication Methods
Facial recognition
MIFARE card authentication
QR code authentication
Multi-factor authentication support
Facial Recognition Technology
Deep learning-based face recognition engine
Dual-lens wide-angle camera system
2 MP image resolution
Advanced anti-spoofing technology preventing access using photographs or other non-live facial images
Face recognition in low-light and complete darkness with adjustable LED illumination
Recognition distance: 0.3 m to 3 m
Recognition time: less than 0.2 seconds
Health and Safety Functions
Face mask detection
Configurable mask compliance policy with optional access denial or access permission
Real-time notifications for non-compliance
Display
7-inch HD LCD capacitive touchscreen
Resolution: 1024 × 600 pixels
Customizable promotional and informational display screens
Audio and Communication
Built-in microphone and speaker
Two-way audio communication
Integration with IP intercom systems
Subscriber calling directly from the terminal
Database Capacity
Up to 6,000 facial templates
Up to 6,000 MIFARE cards
Event storage capacity up to 50,000 records
Network and Interfaces
10/100/1000 Mbps Ethernet interface
RS-485 communication port
Wiegand interface
2 × USB ports
2 alarm inputs
1 alarm output
2-pin power interface
Access Control Features
Door lock control
Exit button connection
Door status sensor connection
Remote door opening
Real-time monitoring and management
Event logging and audit trail
Standalone operation capability without external controller
Video Integration
Recording to Network Video Recorder (NVR)
Real-time video viewing
Integration with video surveillance platforms
Operating System
Embedded Linux operating system
Power Supply
12 VDC, 2 A
Environmental
IP65-rated dust and water protection
Operating temperature: -30°C to +60°C
Physical Characteristics
Dimensions: 239 × 117 × 33 mm
Applications
Office buildings
Industrial facilities
Educational institutions
Hotels and hospitality facilities
Critical infrastructure
Government and commercial facilities
Time attendance and workforce management systems
Warranty
3-year manufacturer warranty
	buc.
	3

	2. 
	Monitor pentru Deschidere de la distanta cu parametrii minim
10.1" IP Indoor Touchscreen Control Monitor for Video Intercom and Security Management
Advanced indoor IP control monitor featuring a 10.1-inch color touchscreen display and Android-based operating system. Designed for integrated management of video intercom, video surveillance, intrusion alarm and access control systems through a single user interface.
Display
10.1-inch color IPS capacitive touchscreen
Resolution: 1024 × 600 pixels
User-friendly graphical interface
LED status illumination integrated into the lower edge of the monitor
Operating System and Applications
Android-based operating system
Pre-installed security management application
Centralized access to connected security devices
Support for installation of third-party Android applications
Integrated management of video surveillance, intercom and alarm systems
Video Functions
Live video viewing from IP cameras
Playback of recorded video archives
Reception of video alarm verification clips from intrusion alarm systems
Real-time monitoring of connected security devices
Video Intercom Functions
Video call reception from outdoor stations
Two-way audio communication
Remote door release functionality
Mobile application integration for receiving and answering calls remotely
Door unlocking from mobile devices and monitor interface
Dedicated physical door release button
Audio
Built-in microphone and speaker
Full duplex two-way communication
Noise suppression technology
Echo cancellation technology
Memory
Internal storage: 8 GB
RAM: 1 GB
Interfaces
10/100 Mbps Ethernet interface
Wi-Fi 802.11 b/g/n
RS-485 communication interface
8 alarm inputs
2 alarm outputs
Tamper protection input
Power Supply
12 VDC power input
Maximum power consumption: 8 W
IEEE 802.3af PoE support
Environmental
Operating temperature range: -10°C to +50°C
Physical Characteristics
Dimensions: 254 × 166 × 27 mm
Applications
Residential buildings
Office and commercial facilities
Hotels and hospitality environments
Integrated security management systems
Access control and video intercom installations
Building Management Systems (BMS)
Package Contents
Indoor monitor unit
Power supply not included
Warranty
3-year manufacturer warranty

	buc
	2

	
	Detectoare

	3. 
	 Detector Magnetic Pentru usi Metalice
	set
	3

	
	Surse de alimentare de rezerva și cutii


	4. 
	Sursa de Alimentare 12V/5A cu acumulator
	Set
	3

	
	Baterii

	
	Cabluri

	
	Structuri de Cablare, Materiale de fixare si lucrari Considerate in Sistemul De Supraveghere Video





Cerinţe privind caracteristicile tehnice

Pentru fiecare echipament în parte se vor livra accesoriile şi cablurile de conexiune necesare 
funcţionării şi interconectării acestora, indiferent dacă acestea au fost sau nu expres solicitate. 
Sistemul va asigura stocarea informațiilor conform normativelor în vigoare, dar nu mai puțin de 
30 zile. 
Accesul la camerele de supraveghere din aplicația mobilă vor deține 3 persoane responsabile.  
 	Este strict necesar de a instala sistemul de supraveghere video cu posibilitatea evitării conflictului  cu rețeaua locală. Sistemul video va fi configurat astfel ca sa permita securizarea perimetrului si teritoriului si va oferi posibilitatea transmiterii acceslui catre agentie de paza care va prelua sistemul ca un sistem complet de paza video. 
Sistemul va asigura supravegherea video pe timp de zi şi de noapte a intrărilor/ ieşirilor din/în 
clădirea instituţiei astfel încât să se realizeze detecţia şi identificarea oricărei încercări de 
pătrundere neautorizată în instituţie, precum şi monitorizarea acceselor autorizate în încăperile 
instituţiei. Sistemul dotat cu centrala biometrica va permite blocarea si securizarea intrarilor pe teritoriul institutiei si accesul pe teritoriul doar a persoanelor autorizate pe baza de date biometrice sau coduri tip QR.





