Pentru achiziționarea imprimantelor

**Cerințe minime obligatorii**

|  |
| --- |
| (new, not refubrished) |
|   | **Type:** | Printer/Scanner/Copier/Fax |
|   | **Technology:** | Laser |
|  | **Control panel:** | Yes (colour touchscreen) |
|  | **Duplex:** | Yes  |
|  | **ADF Type:** | DADF – scan both sides of the page at once |
|   | **Duty cycle (monthly, A4):** | min. 80 000 pages |
| **PRINT** |
|   | **Print speed (min):** | 30 ppm (A4 normal); 30 ipm (A4 duplex). |
|  | **Print resolution:** | min. 600x600 dpi  |
|  | **Standard print languages:** | PCL6, Adobe PostScript3; PDF; Native Office, URF. |
|  | **Print features:** | Print from USB; Print two sides. |
| **COPY** |
|  | **Copy speed (min):** | 35 cpm  |
|  | **Copy Features:** | Automatic Two-Sided; Density Adjustment of image; Multiple Copies (up to 999); Resize. |
| **SCAN** |
|  | **Scan speed (min):** | 35 ipm (single side) |
|  | **Scan file format:** | PDF, JPG, TIFF |
|  | **Scan type:** | Flatbed, DADF 50 sheets; two-sided scanning; Skip Blank Pages; Edge Erase; |
|  | **Scan resolution:** | min. 600x600 dpi |
|  | **Scan features:** | Scan to USB, email LDAP, network folder, computer, Microsoft SharePoint® |
| **OTHER** |
|   | **Memory:** | min. 1024 MB; |
|   | **Processor speed** | Min. 800MHZ; |
|   | **Interfaces:** | Gigabit Ethernet port, min. 1 rear host port; min. 1 front USB port. |
|   | **Paper handling** | Min. 350 sheet A4 input tray. |
|   | **Paper weight:** | Min. 60g/m2 and min. up to 120g/m2 |
|  | **OS Compatibility** | Win 10, Win 8.1, Win 7, Mac OS. |
|   | **Cartridges included:** | Standard cartridge 3000 pages A4; |
|   | **Warranty:** |  Min. 3 Years On-site official manufacturer warranty |