  Unofficial translation from Romanian to English

PARTICIPATION NOTICE
regarding the purchase of Used buses
through the Open tender procurement procedure
The procurement procedure is applied under the incidence of the normative act: 
* Law on procurement in the energy, water, transport and postal services sectors 74/2020
1. Name of the contracting entity: Î.M. Parcul urban de autobuze
2. IDNO: 1004600054327
3. Adresa: mun. Chișinău, str. Sarmizegetusa 51 
4. Telephone/fax number:: 022-83-73-35/022-55-60-30
5. E-mail and internet address of the contracting entity:: achizitii.pua@gmail.com /www.autourban.md
6. E-mail or internet address from which access to the award documentation can be obtained: The award documentation is attached within the procedure in SIA RSAP. 
7. Type of contracting entity and main object of activity (if applicable, the mention that the contracting entity is a central purchasing body or that the procurement involves another form of joint procurement): Sectoral activities regarding the transport field
8. The buyer invites interested economic operators, who can satisfy its needs, to participate in the procurement procedure regarding the delivery/provision/execution of the following goods/services/works:

	


Nr. d/o
	CPV
Cod
	
Name of the requested goods
	Unit of measurement
	Quantity
	Full requested technical specification, reference standards
	Total estimated value without VAT

	 

1
	         Lotul 1

	
	   34121100-2
	

Used buses, category M3
	

pcs
	

21
	

According to the specifications book (attached)
	


38 000 000,00

	Total estimated value, without VAT
	38 000 000,00 MDL



9. If the contract is divided into lots, an economic operator can submit the tender (to be selected): 
1) for a single lot
10. Admission or prohibition of alternative tenders: not admitted.
11. Requested terms and conditions of delivery/provision/execution: The delivery of goods shall be made to the recipient's headquarters in Chișinău, 51 Sarmizegetusa street under DAP conditions (uncleared), all transport expenses being included in the price. Payment will be made in advance, at the time of confirming that the entire lot is ready for delivery, or in installments (for partial deliveries) within up to 10 days. Delivery term: maximum 30 days from the signing of the contract.
Special evaluation condition: Before adopting the contract award decision, the contracting entity has the right to delegate its representatives to the location of the buses to carry out the evaluation of their technical condition and to physically verify the original documents. This documentary verification will include, but will not be limited to: matching the identification number (VIN) on the chassis with the one indicated in the vehicle identity card (brief/technical passport), confirming the authenticity of the maintenance history and service documents to validate the real mileage (running), certifying the pollution norm (ecological class) from the official documents and ensuring the absence of any prohibitions or legal encumbrances on the vehicles.
12. Validity term of the contract: 12 months.
13. Procurement contract reserved for sheltered workshops or that it can be executed only within some sheltered employment programs (if applicable): not applicable.
14. The provision of the service is reserved to a certain profession pursuant to some laws or administrative acts (if applicable): not applicable.
15. Short description of the criteria regarding the eligibility of economic operators that can determine their elimination and of the selection criteria; the minimum level (minimum levels) of the requirements possibly imposed; the requested information is mentioned (ESPD, documentation):
	Nr. d/o
	Description of the criterion/requirement
	Method of demonstrating the fulfillment of the criterion/requirement:
	Minimum level/Mandatory status

	1
	ESPD  Form
	ESPD  Form, electronic signature
	Mandatory

	2
	Price specification  Form
	Price specification  Form, electronic signature
	Mandatory

	3
	Technical specification  Form,
	Technical specification  Form, electronic signature
	Mandatory

	4 
	Certificate of assignment of the bank account issued by the account holding bank
	Certificate of assignment of the bank account issued by the account holding bank , electronic signature
	Mandatory

	5
	Demonstration of the economic operator's experience in the field of activity related to the object of the contract to be awarded  Declaration regarding similar experience.
	Demonstration of the economic operator's experience in the field of activity related to the object of the contract to be awarded  Declaration regarding similar experience. The cumulative value of all contracts executed in the last 3 years of activity must be equal to or greater than the value of the future contract. Copies of the contracts and documents attesting their fulfillment confirmed by applying the tenderer's electronic signature are presented.
	Mandatory

	6
	Information regarding the fulfillment of obligations to pay taxes, duties and social insurance contributions  Copy of the SFS certificate regarding the absence or existence of arrears towards the national public budget, confirmed by the electronic signature of the economic operator
	Information regarding the fulfillment of obligations to pay taxes, duties and social insurance contributions  Copy of the SFS certificate regarding the absence or existence of arrears towards the national public budget, confirmed by the electronic signature of the economic operator
	Mandatory

	7
	Informative form about the tenderer
	Informative form about the tenderer
	Mandatory

	8
	Declaration regarding beneficial owners
	Declaration regarding beneficial owners
	Mandatory

	9
	Extract from the State Register of legal entities
	Extract from the State Register of legal entities
	Mandatory

	10
	Tender guarantee 1%

	a) The tender will be accompanied by a Tender guarantee (issued by a commercial bank)

or

b) Transfer to the account of the contracting entity, according to the following bank details:
Payment beneficiary: Î.M. "Parcul Urban de Autobuze"
Bank details: MOLDMD2X308, BC "Moldindconbank" SA, Dacia branch, Chișinău
Fiscal code: 1004600054327
Settlement account: MD17ML000000002251308233
VAT Code: 0300138
with the note “Tender guarantee” or “For the performance guarantee at the sectoral procurement procedure no. ”According to SIA RSAP” 
	Mandatory

	11
	Performance guarantee 5% of the tender value 
	5% of the tender value.
Form of the performance guarantee:
a) Performance guarantee (issued by a commercial bank)
or
b) Performance guarantee by transfer to the account of the contracting entity, according to the following bank details:
Payment beneficiary: Î.M. "Parcul urban de autobuze"
Fiscal code: 1004600054327
IBAN: MD17ML000000002251308233
VAT Code: 0300138
with the note “For the performance guarantee at the sectoral procurement procedure no. ”According to SIA RSAP”
	Upon awarding the contract  

	12
	Copy of Registration Certificate (Technical Passport / Brief) and/or Vehicle Certificate of Conformity
	Document must explicitly confirm manufacture date to comply with RM customs law regarding import of vehicles maximum 10 years old (inclusive) to avoid extra excise duties.
	Mandatory


16. Reason for accelerated procedure: Not applicable.
17. Specific award techniques/instruments (Framework agreement, DPS, Electronic auction): Not applicable. 
18. Special performance conditions: Not applicable.
19. Contract award criterion: Lowest price, provided all qualification criteria are fully met (100% weight). 
19.1. Tie-breaking criterion (identical pricing): If two or more top-ranked bidders offer identical pricing, the contracting entity will request new financial offers for tie-breaking. The contract will be awarded to the bidder offering the lowest price after re-bidding.
20. Criteria for evaluating the most economically advantageous bid, along with their weightings:
	Nr. d/o
	Name of Evaluation Criterion
	Weighting (%)

	1
	  Lowest price    
	100%



21. Deadline for submission/opening of offers: According to SIA RSAP, via www.achizitii.md  
22. Submission address: Electronically via SIA RSAP.
23. [bookmark: _GoBack]Bid validity period: 30 days.
24. Place of opening: SIA RSAP.
25. Persons Authorized to Attend the Opening of Bids: Bidders or their representatives have the right to attend the opening of bids, unless the bids were submitted through SIA “RSAP.”
26. Languages for tender submission: Romanian and/or English, Russian. 
27. EU funding reference: Not applicable. 
28. Appeals body: National Authority for Dispute Settlement (ANSC), mun. Chișinău, 124 Ștefan cel Mare și Sfânt blvd. (4th floor), MD 2001. Tel/Fax/email: 022 820652, 022 820651, contestatii@ansc.md
29. Date(s) and reference(s) of previous publications in the Official Journal of the European Union regarding the contract(s) to which this notice relates (if applicable): –
30. In the case of periodic procurements, the estimated timing for the publication of future notices: –
31. Publication date of the prior information notice or, where applicable, an indication that no such notice was published: –
32. Date of dispatch of the contract notice for publication: Reflected in SIA RSAP
33. The following electronic tools will be used/accepted within the public procurement procedure:
	Name of the electronic tool
	Will be used/accepted or not

	Electronic submission of tenders or requests to participate
	Will be used

	Electronic ordering system
	Will not be used

	Electronic invoicing
	Will be used (if applicable)

	Electronic payments
	Will not be used


34. The contract is covered by the World Trade Organization Agreement on Government Procurement (only in the case of notices dispatched for publication in the Official Journal of the European Union): Not applicable.
35. NUTS code of the main place of execution of works, in the case of works, or the NUTS code of the main place of delivery or performance, in the case of goods and services (to be indicated for utilities/sectoral procurements): MD 115
36. Information on the requested guarantees: Not applicable.
37. Other relevant information:
· All requested documents must be uploaded to SIA RSAP "MTender" prior to the deadline for tender submission; otherwise, the tender will be rejected.
· The performance guarantee shall be returned by I.M. "Parcul urban de autobuze" upon full execution of the sectoral procurement contract.
· The bidder whose tender is designated as winning shall sign the sectoral procurement contract within 10 days from the date it was sent to them for signature.
· If, upon expiry of the period specified above, the bidder who received the notice of acceptance has not signed the sectoral procurement contract or has not provided the performance guarantee, the contracting entity shall reject the tender and award the contract to the next ranked bidder, provided that their tender remains valid.
Chairman of the Working Group 
for Public Procurement of Goods, Works, and Services:                                      Zadeseneț Ghenadie









TERMS OF REFERENCE
for the purchase of 21 used (pre-owned) buses

1. The present terms of reference establish the minimum technical, qualitative, and performance conditions for the purchase of 21 used buses. The buses are intended for the public transport of passengers on urban/suburban routes and must ensure a high level of safety, comfort, and reliability.
To ensure the efficiency of subsequent operation and maintenance, the purchase will be guided by the following principles and mandatory requirements:
· supply of all 21 buses by a single seller;
· formation of a homogeneous lot, mainly of buses of the same brand, model, and manufacturer;
· compliance with mandatory technical characteristics;
· lowest total price, without VAT, including transport to Chișinău under DAP conditions (duty unpaid);
· avoidance of additional expenses related to the import of buses older than 10 years inclusive.
2. Mandatory Minimum Technical Specifications
The bidder must ensure compliance with the following technical specifications for each of the 21 delivered units:
	Nr. d/o
	Description
	Requirements

	1
	General characteristics

	1.1
	Year of manufacture
	Maximum year 2016

	1.2
	Vehicle category
	M3, Bus for passenger transport on urban and suburban routes, at an ambient temperature from minus 35 °C to plus 45 °C

	1.3
	Ecological class
	Minimum Euro 5

	1.4
	Total capacity, passengers
	Minimum 150 (including driver)

	1.5
	Number of seating places, including driver and persons with special needs
	Minimum 50

	1.6
	Number of seating places for persons with special needs
	Minimum 1

	1.7
	Climbing gradient supported by the bus with maximum permissible load, not less than
	25%

	1.8
	Turning radius, not more than
	12.5 m

	1.9
	Drive axle
	Rear

	1.10
	Mileage, km
	Maximum 800,000

	1.11
	Tires
	Tubeless

	1.12
	Overall dimensions:
- length, mm
- width, mm
- height, mm
	
minimum 18,000, maximum 18,750
maximum 2,550
maximum 3,350

	1.13
	Ground clearance, mm
	not less than 130

	1.14
	Floor level, mm
	maximum 340

	1.15
	Floor level upon activation of the kneeling system at stops, kneeling mm
	maximum 270

	1.16
	Floor level
	Low floor along the entire length of the bus

	2
	                                                Bus bodywork

	2.1
	Body type
	Body with anti-corrosion treatment.

	2.2
	Number of doors
	Minimum 3 with double leaves (2+2+2)

	2.3
	Subflooring
	SubflooringResistant to wear and rot

	2.4
	Floor covering
	Waterproof, resistant to frictional wear.

	2.5
	Bus interior
	- It must be equipped with a sufficient number of handrails for maximum safe transport of passengers;
- mechanical, folding ramp for access of persons with reduced mobility.

	2.6
	Passenger seats
	Vandal-resistant, semi-rigid with anti-trauma handle.

	2.7
	Ventilation and heating system:
	Air conditioning system with a minimum power of 39 kW. Driver's cabin heating – autonomous heating (pre-heater with a minimum power of at least 24 kW).

	2.8
	Driver's workplace
	The cabin will be equipped with ventilation through the side window, air conditioning. Driver's seat – pneumatic suspension with height adjustment of the seat cushion, longitudinal position, backrest inclination angle. Triplex-type windshield.

	2.9
	Exterior rearview mirrors
	Heated and electrically operated.

	2.10
	Information system
	Onboard electronic route informer (front, side, rear) with information broadcast via USB stick or analog; interior informer with microphone and speakers.

	2.11
	Towing device
	The bus must be equipped with a towing device at the front and rear.

	2.12
	Video surveillance system
	Passenger interior + rear

	2.13
	Passenger information system
	Minimum 2 monitors in the passenger cabin

	3
	Technical characteristics
	

	3.1
	Engine
	Four-stroke diesel engine with turbocharger.

	3.2
	Cooling system
	Closed-type liquid circulation.

	3.3
	Engine power, kW
	Min. 260 kW

	3.4
	Gearbox
	Automatic with retarder.

	3.5
	Front axle
	Dependent or independent

	3.6
	Rear axle
	Banjo/crankcase-type rear axle with axle reducer.

	3.7
	Front suspension
	Dependent with two pneumatic elements, two hydraulic shock absorbers, and air level regulator.

	3.8
	Rear suspension
	Dependent, with four pneumatic elements, four hydraulic shock absorbers, and air level regulator.

	3.9
	Steering system
	Integral type, adjustable steering column, anti-trauma.

	3.10
	Braking system
	Pneumatic, with discs on all axles, ABS, ASR, EBS system.

	3.11
	Electrical equipment
	Batteries – 2 min 225 Ah

	3.12 
	Tires
	275/70 R 22.5


3. Accompanying documents upon delivery: Upon delivery, each bus shall be accompanied by:
· Vehicle identity card (Original technical Brief) from the country of origin.
· Documents necessary for customs clearance and registration in the Republic of Moldova.
· Maintenance history (Service book or extract from the previous operator's database) attesting the truthfulness of the mileage.
· Vehicle user/operation manual.
· Spare parts catalog for the offered model.

4. Reception of the buses: The reception will be carried out at the headquarters of the Contracting Entity by a reception commission. The commission will verify the technical condition, the functionality of all equipment (especially the air conditioning, the ramp, and the condition of the engine/gearbox), and compliance with these terms of reference. In case defects are detected, the supplier is obliged to remedy them at its own expense within a maximum of 15 working days.

Note: All specifications in these terms of reference are considered mandatory minimum requirements. Tenders that do not comply with these requirements will be disqualified.

Chairman of the Procurement Working Group 
for Public Procurement of Goods, Works, and Services: ______________________ Zadeseneț Ghenadie


